


**DATE SUBMITTED: 11/7/18**


**Task 1**


|  |
| --- |
| //--------------------------------------------------------------------------------- // Project: Blink TM4C BIOS Using Hwi (STARTER) // Author: Eric Wilbur // Date: June 2014 // // Note: The function call TimerIntClear(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT) HAS // to be in the ISR. This fxn clears the TIMER's interrupt flag coming // from the peripheral - it does NOT clear the CPU interrupt flag - that // is done by hardware. The author struggled figuring this part out - hence // the note. And, in the Swi lab, this fxn must be placed in the // Timer\_ISR fxn because it will be the new ISR. // // Follow these steps to create this project in CCSv6.0: // 1. Project -> New CCS Project // 2. Select Template: // - TI-RTOS for Tiva-C -> Driver Examples -> EK-TM4C123 LP -> Example Projects -> // Empty Project // - Empty Project contains full instrumentation (UIA, RTOS Analyzer) and // paths set up for the TI-RTOS version of MSP430Ware // 3. Delete the following files: // - Board.h, empty.c, EK\_TM4C123GXL.c/h, empty\_readme.txt // 4. Add main.c from TI-RTOS Workshop Solution file for this lab // 5. Edit empty.cfg as needed (to add/subtract) BIOS services, delete given Task // 6. Build, load, run... //----------------------------------------------------------------------------------   //---------------------------------------- // BIOS header files //---------------------------------------- #include <xdc/std.h> //mandatory - have to include first, for BIOS types #include <ti/sysbios/BIOS.h> //mandatory - if you call APIs like BIOS\_start() #include <xdc/runtime/Log.h> //needed for any Log\_info() call #include <xdc/cfg/global.h> //header file for statically defined objects/handles   //------------------------------------------ // TivaWare Header Files //------------------------------------------ #include <stdint.h> #include <stdbool.h>  #include "inc/hw\_types.h" #include "inc/hw\_memmap.h" #include "driverlib/sysctl.h" #include "driverlib/gpio.h" #include "inc/hw\_ints.h" #include "driverlib/interrupt.h" #include "driverlib/timer.h"   //---------------------------------------- // Prototypes //---------------------------------------- void hardware\_init(void); void ledToggle(void); void delay(void);   //--------------------------------------- // Globals //--------------------------------------- volatile int16\_t i16ToggleCount = 0;   //--------------------------------------------------------------------------- // main() //--------------------------------------------------------------------------- void main(void) {   hardware\_init(); // init hardware via Xware   BIOS\_start();  }   //--------------------------------------------------------------------------- // hardware\_init() // // inits GPIO pins for toggling the LED //--------------------------------------------------------------------------- void hardware\_init(void) {  uint32\_t ui32Period;   //Set CPU Clock to 40MHz. 400MHz PLL/2 = 200 DIV 5 = 40MHz  SysCtlClockSet(SYSCTL\_SYSDIV\_5|SYSCTL\_USE\_PLL|SYSCTL\_XTAL\_16MHZ|SYSCTL\_OSC\_MAIN);   // ADD Tiva-C GPIO setup - enables port, sets pins 1-3 (RGB) pins for output  SysCtlPeripheralEnable(SYSCTL\_PERIPH\_GPIOF);  GPIOPinTypeGPIOOutput(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3);   // Turn on the LED  GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 4);   // Timer 2 setup code  SysCtlPeripheralEnable(SYSCTL\_PERIPH\_TIMER2); // enable Timer 2 periph clks  TimerConfigure(TIMER2\_BASE, TIMER\_CFG\_PERIODIC); // cfg Timer 2 mode - periodic   ui32Period = (SysCtlClockGet() /2); // period = CPU clk div 2 (500ms)  TimerLoadSet(TIMER2\_BASE, TIMER\_A, ui32Period); // set Timer 2 period   TimerIntEnable(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT); // enables Timer 2 to interrupt CPU   TimerEnable(TIMER2\_BASE, TIMER\_A); // enable Timer 2  }   //--------------------------------------------------------------------------- // ledToggle() // // toggles LED on Tiva-C LaunchPad //--------------------------------------------------------------------------- void ledToggle(void) {  TimerIntClear(TIMER2\_BASE, TIMER\_TIMA\_TIMEOUT); // must clear timer flag FROM timer   // LED values - 2=RED, 4=BLUE, 8=GREEN  if(GPIOPinRead(GPIO\_PORTF\_BASE, GPIO\_PIN\_2))  {  GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_1|GPIO\_PIN\_2|GPIO\_PIN\_3, 0);  }  else  {  GPIOPinWrite(GPIO\_PORTF\_BASE, GPIO\_PIN\_2, 4);  }   //delay(); // create a delay of ~1/2sec   i16ToggleCount += 1; // keep track of #toggles   Log\_info1("LED TOGGLED [%u] TIMES",i16ToggleCount); // send toggle count to UIA  }   //--------------------------------------------------------------------------- // delay() // // Creates a 500ms delay via TivaWare fxn //--------------------------------------------------------------------------- //void delay(void) //{ // SysCtlDelay(6700000); // creates ~500ms delay - TivaWare fxn // //} |







****

****

****



****

**Youtube Link:** <https://youtu.be/-RdRrCx7GOw>